Complete units come with a geyser tank, evacuated tubes and stand. Just assemble & connect piping. These SM types can be used on high pressure as well, via e.g. Lacto valves! (NORMALLY Standard elements can be connected **IF** NECESSARY).

·         The manifold system fits on an existing (in-roof) geyser tank & usually has a specialized SM 12/24 volt solar powered circulation pump DC solar panel(s) that drives the pump. (SM systems does not incl glycol). SM tanker controllers (normally thermo heat exchange compatible, into elements...) can be used to control water temp... in e.g. tanks etc! (In general!)